Dimensions of PROTEUS:

* VLA has 18 channels with 3 m spacing (spans 68.5-17.5m depth in 74 m water)
* HLA has 34 channels that extends 140 m with a center taper as shown in the figure below

A diagram of a line array

Description automatically generated

Image from “Sagers\_PROTEUS Seabed Workshop 2021.08.02 v2.pptx”

Sampling rate: 10,240 Hz

-168 dB sensitivity on all channels except VLA 1, 4, 7, 10, 13, & 16 which had -220 dB sensitivity

Recordings go from 7 May 03:00 UTC – 3 Jun 12:00 UTC. (Data goes from 20220507.025421 to 20220603.125550 in the format YYYYMMDD.HHMMSS).